# Copyright (C) 1991-2005 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.


# The default values for assignments are stored in the file
#		standard_assignment_defaults.qdf
# If this file doesn't exist, and for assignments not listed, see file
#		assignment_defaults.qdf

# Altera recommends that you do not modify this file. This
# file is updated automatically by the Quartus II software
# and any changes you make may be lost or overwritten.


set_global_assignment -name FAMILY Cyclone
set_global_assignment -name DEVICE EP1C20F400C7
set_global_assignment -name TOP_LEVEL_ENTITY standard
set_global_assignment -name RESERVE_ALL_UNUSED_PINS "AS INPUT TRI-STATED"
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 5.1
set_global_assignment -name PROJECT_CREATION_TIME_DATE "13:33:11  SEPTEMBER 07, 2005"
set_global_assignment -name LAST_QUARTUS_VERSION 6.0
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR 1
set_global_assignment -name RESERVE_PIN "AS INPUT TRI-STATED"
set_location_assignment PIN_J13 -to CTS[1]
set_location_assignment PIN_M16 -to DCD[1]
set_location_assignment PIN_M20 -to DSR[1]
set_location_assignment PIN_M15 -to DTR[1]
set_location_assignment PIN_V7 -to out_port_from_the_seven_seg_pio[0]
set_location_assignment PIN_T6 -to out_port_from_the_seven_seg_pio[10]
set_location_assignment PIN_W5 -to out_port_from_the_seven_seg_pio[11]
set_location_assignment PIN_V5 -to out_port_from_the_seven_seg_pio[12]
set_location_assignment PIN_U5 -to out_port_from_the_seven_seg_pio[13]
set_location_assignment PIN_T5 -to out_port_from_the_seven_seg_pio[14]
set_location_assignment PIN_Y6 -to out_port_from_the_seven_seg_pio[15]
set_location_assignment PIN_T8 -to out_port_from_the_seven_seg_pio[1]
set_location_assignment PIN_R7 -to out_port_from_the_seven_seg_pio[2]
set_location_assignment PIN_Y7 -to out_port_from_the_seven_seg_pio[3]
set_location_assignment PIN_W7 -to out_port_from_the_seven_seg_pio[4]
set_location_assignment PIN_V6 -to out_port_from_the_seven_seg_pio[5]
set_location_assignment PIN_U6 -to out_port_from_the_seven_seg_pio[6]
set_location_assignment PIN_U7 -to out_port_from_the_seven_seg_pio[7]
set_location_assignment PIN_W6 -to out_port_from_the_seven_seg_pio[8]
set_location_assignment PIN_T7 -to out_port_from_the_seven_seg_pio[9]
set_location_assignment PIN_A14 -to ENET_ADS_N
set_location_assignment PIN_B15 -to ENET_AEN
set_location_assignment PIN_C16 -to byteenablen_to_the_lan91c111[0]
set_location_assignment PIN_B16 -to byteenablen_to_the_lan91c111[1]
set_location_assignment PIN_D16 -to byteenablen_to_the_lan91c111[2]
set_location_assignment PIN_E16 -to byteenablen_to_the_lan91c111[3]
set_location_assignment PIN_B17 -to ENET_CYCLE_N
set_location_assignment PIN_C15 -to ENET_DATACS_N
set_location_assignment PIN_D15 -to irq_from_the_lan91c111
set_location_assignment PIN_F14 -to ardy_from_the_lan91c111
set_location_assignment PIN_A15 -to ior_n_to_the_lan91c111
set_location_assignment PIN_E15 -to iow_n_to_the_lan91c111
set_location_assignment PIN_C17 -to ENET_LCLK
set_location_assignment PIN_D3 -to ENET_LDEV_N
set_location_assignment PIN_B18 -to ENET_RDYRTN_N
set_location_assignment PIN_M8 -to ENET_SRDY_N
set_location_assignment PIN_A17 -to ENET_W_R_N
set_location_assignment PIN_A12 -to select_n_to_the_ext_flash
set_location_assignment PIN_B12 -to read_n_to_the_ext_flash
set_location_assignment PIN_D12 -to write_n_to_the_ext_flash
set_location_assignment PIN_C12 -to FLASH_RY_BY_N
set_location_assignment PIN_B4 -to ext_ram_bus_address[0]
set_location_assignment PIN_E4 -to ext_ram_bus_address[10]
set_location_assignment PIN_E5 -to ext_ram_bus_address[11]
set_location_assignment PIN_F3 -to ext_ram_bus_address[12]
set_location_assignment PIN_E3 -to ext_ram_bus_address[13]
set_location_assignment PIN_E2 -to ext_ram_bus_address[14]
set_location_assignment PIN_F4 -to ext_ram_bus_address[15]
set_location_assignment PIN_F5 -to ext_ram_bus_address[16]
set_location_assignment PIN_F2 -to ext_ram_bus_address[17]
set_location_assignment PIN_F1 -to ext_ram_bus_address[18]
set_location_assignment PIN_F6 -to ext_ram_bus_address[19]
set_location_assignment PIN_A4 -to ext_ram_bus_address[1]
set_location_assignment PIN_G5 -to ext_ram_bus_address[20]
set_location_assignment PIN_G1 -to ext_ram_bus_address[21]
set_location_assignment PIN_G2 -to ext_ram_bus_address[22]
set_location_assignment PIN_D5 -to ext_ram_bus_address[2]
set_location_assignment PIN_D6 -to ext_ram_bus_address[3]
set_location_assignment PIN_C5 -to ext_ram_bus_address[4]
set_location_assignment PIN_B5 -to ext_ram_bus_address[5]
set_location_assignment PIN_C2 -to ext_ram_bus_address[6]
set_location_assignment PIN_D2 -to ext_ram_bus_address[7]
set_location_assignment PIN_D4 -to ext_ram_bus_address[8]
set_location_assignment PIN_D1 -to ext_ram_bus_address[9]
set_location_assignment PIN_C6 -to ext_ram_bus_data[0]
set_location_assignment PIN_F8 -to ext_ram_bus_data[10]
set_location_assignment PIN_E8 -to ext_ram_bus_data[11]
set_location_assignment PIN_B8 -to ext_ram_bus_data[12]
set_location_assignment PIN_A8 -to ext_ram_bus_data[13]
set_location_assignment PIN_D8 -to ext_ram_bus_data[14]
set_location_assignment PIN_C8 -to ext_ram_bus_data[15]
set_location_assignment PIN_B9 -to ext_ram_bus_data[16]
set_location_assignment PIN_A9 -to ext_ram_bus_data[17]
set_location_assignment PIN_D9 -to ext_ram_bus_data[18]
set_location_assignment PIN_C9 -to ext_ram_bus_data[19]
set_location_assignment PIN_E6 -to ext_ram_bus_data[1]
set_location_assignment PIN_E9 -to ext_ram_bus_data[20]
set_location_assignment PIN_E10 -to ext_ram_bus_data[21]
set_location_assignment PIN_B10 -to ext_ram_bus_data[22]
set_location_assignment PIN_A10 -to ext_ram_bus_data[23]
set_location_assignment PIN_F10 -to ext_ram_bus_data[24]
set_location_assignment PIN_C10 -to ext_ram_bus_data[25]
set_location_assignment PIN_D10 -to ext_ram_bus_data[26]
set_location_assignment PIN_C11 -to ext_ram_bus_data[27]
set_location_assignment PIN_D11 -to ext_ram_bus_data[28]
set_location_assignment PIN_B11 -to ext_ram_bus_data[29]
set_location_assignment PIN_B6 -to ext_ram_bus_data[2]
set_location_assignment PIN_A11 -to ext_ram_bus_data[30]
set_location_assignment PIN_E11 -to ext_ram_bus_data[31]
set_location_assignment PIN_A6 -to ext_ram_bus_data[3]
set_location_assignment PIN_F7 -to ext_ram_bus_data[4]
set_location_assignment PIN_E7 -to ext_ram_bus_data[5]
set_location_assignment PIN_B7 -to ext_ram_bus_data[6]
set_location_assignment PIN_A7 -to ext_ram_bus_data[7]
set_location_assignment PIN_D7 -to ext_ram_bus_data[8]
set_location_assignment PIN_C7 -to ext_ram_bus_data[9]
set_location_assignment PIN_C3 -to INIT_DONE
set_location_assignment PIN_H14 -to LCD_data_to_and_from_the_lcd_display[0]
set_location_assignment PIN_J14 -to LCD_data_to_and_from_the_lcd_display[1]
set_location_assignment PIN_J17 -to LCD_data_to_and_from_the_lcd_display[2]
set_location_assignment PIN_J18 -to LCD_data_to_and_from_the_lcd_display[3]
set_location_assignment PIN_K15 -to LCD_data_to_and_from_the_lcd_display[4]
set_location_assignment PIN_W18 -to LCD_data_to_and_from_the_lcd_display[5]
set_location_assignment PIN_V18 -to LCD_data_to_and_from_the_lcd_display[6]
set_location_assignment PIN_V19 -to LCD_data_to_and_from_the_lcd_display[7]
set_location_assignment PIN_J19 -to LCD_RW_from_the_lcd_display
set_location_assignment PIN_J15 -to LCD_RS_from_the_lcd_display
set_location_assignment PIN_J20 -to LCD_E_from_the_lcd_display
set_location_assignment PIN_E14 -to out_port_from_the_led_pio[0]
set_location_assignment PIN_E13 -to out_port_from_the_led_pio[1]
set_location_assignment PIN_C14 -to out_port_from_the_led_pio[2]
set_location_assignment PIN_D14 -to out_port_from_the_led_pio[3]
set_location_assignment PIN_E12 -to out_port_from_the_led_pio[4]
set_location_assignment PIN_F12 -to out_port_from_the_led_pio[5]
set_location_assignment PIN_B3 -to out_port_from_the_led_pio[6]
set_location_assignment PIN_B14 -to out_port_from_the_led_pio[7]
set_location_assignment PIN_M17 -to jtag_debug_offchip_trace_clk_from_the_cpu
set_location_assignment PIN_P16 -to TR_DEBUGACK
set_location_assignment PIN_M18 -to TR_DEBUGREQ
set_location_assignment PIN_P17 -to jtag_debug_trigout_from_the_cpu
set_location_assignment PIN_U17 -to jtag_debug_offchip_trace_data_from_the_cpu[0]
set_location_assignment PIN_T18 -to jtag_debug_offchip_trace_data_from_the_cpu[1]
set_location_assignment PIN_T19 -to jtag_debug_offchip_trace_data_from_the_cpu[2]
set_location_assignment PIN_T17 -to jtag_debug_offchip_trace_data_from_the_cpu[3]
set_location_assignment PIN_R16 -to jtag_debug_offchip_trace_data_from_the_cpu[4]
set_location_assignment PIN_R19 -to jtag_debug_offchip_trace_data_from_the_cpu[5]
set_location_assignment PIN_R20 -to jtag_debug_offchip_trace_data_from_the_cpu[6]
set_location_assignment PIN_R17 -to jtag_debug_offchip_trace_data_from_the_cpu[7]
set_location_assignment PIN_R18 -to jtag_debug_offchip_trace_data_from_the_cpu[8]
set_location_assignment PIN_R15 -to jtag_debug_offchip_trace_data_from_the_cpu[9]
set_location_assignment PIN_P14 -to jtag_debug_offchip_trace_data_from_the_cpu[10]
set_location_assignment PIN_P18 -to jtag_debug_offchip_trace_data_from_the_cpu[11]
set_location_assignment PIN_P15 -to jtag_debug_offchip_trace_data_from_the_cpu[12]
set_location_assignment PIN_P19 -to jtag_debug_offchip_trace_data_from_the_cpu[13]
set_location_assignment PIN_P20 -to jtag_debug_offchip_trace_data_from_the_cpu[14]
set_location_assignment PIN_N14 -to jtag_debug_offchip_trace_data_from_the_cpu[15]
set_location_assignment PIN_N18 -to jtag_debug_offchip_trace_data_from_the_cpu[16]
set_location_assignment PIN_N17 -to jtag_debug_offchip_trace_data_from_the_cpu[17]
set_location_assignment PIN_L4 -to PLD_ASDO
set_location_assignment PIN_L5 -to PLD_CE_N
set_location_assignment PIN_C4 -to PLD_CLEAR_N
set_location_assignment PIN_L14 -to PLD_CLKFB
set_location_assignment PIN_L8 -to PLD_CLKOUT
set_location_assignment PIN_K5 -to PLD_CLOCKINPUT[1]
set_location_assignment PIN_K2 -to PLD_CS_N
set_location_assignment PIN_K3 -to PLD_DATA[0]
set_location_assignment PIN_L1 -to PLD_MSEL[0]
set_location_assignment PIN_L6 -to PLD_MSEL[1]
set_location_assignment PIN_V8 -to bidir_port_to_and_from_the_reconfig_request_pio
set_location_assignment PIN_K6 -to PROTO1_CLKOUT
set_location_assignment PIN_G15 -to PROTO1_IO[16]
set_location_assignment PIN_G14 -to PROTO1_IO[19]
set_location_assignment PIN_G17 -to PROTO1_IO[22]
set_location_assignment PIN_H16 -to PROTO1_IO[23]
set_location_assignment PIN_J16 -to PROTO1_IO[28]
set_location_assignment PIN_U20 -to PROTO1_IO[40]
set_location_assignment PIN_U8 -to PROTO2_CARDSEL_N
set_location_assignment PIN_K14 -to PROTO2_CLKOUT
set_location_assignment PIN_T15 -to PROTO2_IO[0]
set_location_assignment PIN_R14 -to PROTO2_IO[10]
set_location_assignment PIN_V13 -to PROTO2_IO[11]
set_location_assignment PIN_U13 -to PROTO2_IO[12]
set_location_assignment PIN_W13 -to PROTO2_IO[13]
set_location_assignment PIN_Y13 -to PROTO2_IO[14]
set_location_assignment PIN_R13 -to PROTO2_IO[15]
set_location_assignment PIN_T13 -to PROTO2_IO[16]
set_location_assignment PIN_V12 -to PROTO2_IO[17]
set_location_assignment PIN_U12 -to PROTO2_IO[18]
set_location_assignment PIN_T12 -to PROTO2_IO[19]
set_location_assignment PIN_W15 -to PROTO2_IO[1]
set_location_assignment PIN_T11 -to PROTO2_IO[20]
set_location_assignment PIN_W12 -to PROTO2_IO[21]
set_location_assignment PIN_Y12 -to PROTO2_IO[22]
set_location_assignment PIN_W8 -to PROTO2_IO[23]
set_location_assignment PIN_Y8 -to PROTO2_IO[24]
set_location_assignment PIN_U9 -to PROTO2_IO[25]
set_location_assignment PIN_V9 -to PROTO2_IO[26]
set_location_assignment PIN_T9 -to PROTO2_IO[27]
set_location_assignment PIN_R9 -to PROTO2_IO[28]
set_location_assignment PIN_Y9 -to PROTO2_IO[29]
set_location_assignment PIN_Y15 -to PROTO2_IO[2]
set_location_assignment PIN_W9 -to PROTO2_IO[30]
set_location_assignment PIN_T10 -to PROTO2_IO[31]
set_location_assignment PIN_U10 -to PROTO2_IO[32]
set_location_assignment PIN_V10 -to PROTO2_IO[33]
set_location_assignment PIN_W10 -to PROTO2_IO[34]
set_location_assignment PIN_Y10 -to PROTO2_IO[35]
set_location_assignment PIN_V11 -to PROTO2_IO[36]
set_location_assignment PIN_U11 -to PROTO2_IO[37]
set_location_assignment PIN_W11 -to PROTO2_IO[38]
set_location_assignment PIN_Y11 -to PROTO2_IO[39]
set_location_assignment PIN_U15 -to PROTO2_IO[3]
set_location_assignment PIN_R11 -to PROTO2_IO[40]
set_location_assignment PIN_V15 -to PROTO2_IO[4]
set_location_assignment PIN_V14 -to PROTO2_IO[5]
set_location_assignment PIN_U14 -to PROTO2_IO[6]
set_location_assignment PIN_Y14 -to PROTO2_IO[7]
set_location_assignment PIN_W14 -to PROTO2_IO[8]
set_location_assignment PIN_T14 -to PROTO2_IO[9]
set_location_assignment PIN_M19 -to RI[1]
set_location_assignment PIN_K19 -to RTS[1]
set_location_assignment PIN_K16 -to rxd_to_the_uart1
set_location_assignment PIN_C13 -to rxd_to_the_uart2
set_location_assignment PIN_M2 -to zs_addr_from_the_sdram[0]
set_location_assignment PIN_H6 -to zs_addr_from_the_sdram[10]
set_location_assignment PIN_H5 -to zs_addr_from_the_sdram[11]
set_location_assignment PIN_M1 -to zs_addr_from_the_sdram[1]
set_location_assignment PIN_M6 -to zs_addr_from_the_sdram[2]
set_location_assignment PIN_M4 -to zs_addr_from_the_sdram[3]
set_location_assignment PIN_J8 -to zs_addr_from_the_sdram[4]
set_location_assignment PIN_J7 -to zs_addr_from_the_sdram[5]
set_location_assignment PIN_J6 -to zs_addr_from_the_sdram[6]
set_location_assignment PIN_J5 -to zs_addr_from_the_sdram[7]
set_location_assignment PIN_J4 -to zs_addr_from_the_sdram[8]
set_location_assignment PIN_J3 -to zs_addr_from_the_sdram[9]
set_location_assignment PIN_H7 -to zs_ba_from_the_sdram[0]
set_location_assignment PIN_H1 -to zs_ba_from_the_sdram[1]
set_location_assignment PIN_G3 -to zs_cas_n_from_the_sdram
set_location_assignment PIN_G7 -to zs_cke_from_the_sdram
set_location_assignment PIN_L13 -to SDRAM_CLK
set_location_assignment PIN_G6 -to zs_cs_n_from_the_sdram
set_location_assignment PIN_J2 -to zs_dqm_from_the_sdram[0]
set_location_assignment PIN_J1 -to zs_dqm_from_the_sdram[1]
set_location_assignment PIN_H4 -to zs_dqm_from_the_sdram[2]
set_location_assignment PIN_H3 -to zs_dqm_from_the_sdram[3]
set_location_assignment PIN_M5 -to zs_dq_to_and_from_the_sdram[0]
set_location_assignment PIN_P7 -to zs_dq_to_and_from_the_sdram[10]
set_location_assignment PIN_P2 -to zs_dq_to_and_from_the_sdram[11]
set_location_assignment PIN_P1 -to zs_dq_to_and_from_the_sdram[12]
set_location_assignment PIN_P6 -to zs_dq_to_and_from_the_sdram[13]
set_location_assignment PIN_P5 -to zs_dq_to_and_from_the_sdram[14]
set_location_assignment PIN_P3 -to zs_dq_to_and_from_the_sdram[15]
set_location_assignment PIN_P4 -to zs_dq_to_and_from_the_sdram[16]
set_location_assignment PIN_R1 -to zs_dq_to_and_from_the_sdram[17]
set_location_assignment PIN_R2 -to zs_dq_to_and_from_the_sdram[18]
set_location_assignment PIN_R6 -to zs_dq_to_and_from_the_sdram[19]
set_location_assignment PIN_M3 -to zs_dq_to_and_from_the_sdram[1]
set_location_assignment PIN_R5 -to zs_dq_to_and_from_the_sdram[20]
set_location_assignment PIN_R3 -to zs_dq_to_and_from_the_sdram[21]
set_location_assignment PIN_R4 -to zs_dq_to_and_from_the_sdram[22]
set_location_assignment PIN_T4 -to zs_dq_to_and_from_the_sdram[23]
set_location_assignment PIN_T2 -to zs_dq_to_and_from_the_sdram[24]
set_location_assignment PIN_T3 -to zs_dq_to_and_from_the_sdram[25]
set_location_assignment PIN_U1 -to zs_dq_to_and_from_the_sdram[26]
set_location_assignment PIN_U4 -to zs_dq_to_and_from_the_sdram[27]
set_location_assignment PIN_U2 -to zs_dq_to_and_from_the_sdram[28]
set_location_assignment PIN_U3 -to zs_dq_to_and_from_the_sdram[29]
set_location_assignment PIN_M7 -to zs_dq_to_and_from_the_sdram[2]
set_location_assignment PIN_V3 -to zs_dq_to_and_from_the_sdram[30]
set_location_assignment PIN_V2 -to zs_dq_to_and_from_the_sdram[31]
set_location_assignment PIN_N6 -to zs_dq_to_and_from_the_sdram[3]
set_location_assignment PIN_N1 -to zs_dq_to_and_from_the_sdram[4]
set_location_assignment PIN_N2 -to zs_dq_to_and_from_the_sdram[5]
set_location_assignment PIN_N4 -to zs_dq_to_and_from_the_sdram[6]
set_location_assignment PIN_N3 -to zs_dq_to_and_from_the_sdram[7]
set_location_assignment PIN_N5 -to zs_dq_to_and_from_the_sdram[8]
set_location_assignment PIN_N7 -to zs_dq_to_and_from_the_sdram[9]
set_location_assignment PIN_H2 -to zs_ras_n_from_the_sdram
set_location_assignment PIN_G4 -to zs_we_n_from_the_sdram
set_location_assignment PIN_V17 -to be_n_to_the_ext_ram[0]
set_location_assignment PIN_V16 -to be_n_to_the_ext_ram[1]
set_location_assignment PIN_W16 -to be_n_to_the_ext_ram[2]
set_location_assignment PIN_T16 -to be_n_to_the_ext_ram[3]
set_location_assignment PIN_W17 -to select_n_to_the_ext_ram
set_location_assignment PIN_Y17 -to read_n_to_the_ext_ram
set_location_assignment PIN_U16 -to write_n_to_the_ext_ram
set_location_assignment PIN_M14 -to txd_from_the_uart1
set_location_assignment PIN_A13 -to txd_from_the_uart2
set_location_assignment PIN_W3 -to in_port_to_the_button_pio[0]
set_location_assignment PIN_Y4 -to in_port_to_the_button_pio[1]
set_location_assignment PIN_V4 -to in_port_to_the_button_pio[2]
set_location_assignment PIN_W4 -to in_port_to_the_button_pio[3]
set_location_assignment PIN_B13 -to cf_detect
set_location_assignment PIN_G17 -to cf_intrq
set_location_assignment PIN_G14 -to cf_iordy
set_location_assignment PIN_H17 -to cf_addr[0]
set_location_assignment PIN_H18 -to cf_addr[1]
set_location_assignment PIN_H19 -to cf_addr[2]
set_location_assignment PIN_W18 -to cf_addr[3]
set_location_assignment PIN_K15 -to cf_addr[4]
set_location_assignment PIN_J18 -to cf_addr[5]
set_location_assignment PIN_J17 -to cf_addr[6]
set_location_assignment PIN_J14 -to cf_addr[7]
set_location_assignment PIN_H14 -to cf_addr[8]
set_location_assignment PIN_J20 -to cf_addr[9]
set_location_assignment PIN_J15 -to cf_addr[10]
set_location_assignment PIN_D13 -to cf_atasel
set_location_assignment PIN_H20 -to cf_cs_n[0]
set_location_assignment PIN_U19 -to cf_cs_n[1]
set_location_assignment PIN_F20 -to cf_data[0]
set_location_assignment PIN_F15 -to cf_data[1]
set_location_assignment PIN_E19 -to cf_data[2]
set_location_assignment PIN_F18 -to cf_data[3]
set_location_assignment PIN_E17 -to cf_data[4]
set_location_assignment PIN_D17 -to cf_data[5]
set_location_assignment PIN_D18 -to cf_data[6]
set_location_assignment PIN_C18 -to cf_data[7]
set_location_assignment PIN_C19 -to cf_data[8]
set_location_assignment PIN_D19 -to cf_data[9]
set_location_assignment PIN_D20 -to cf_data[10]
set_location_assignment PIN_F17 -to cf_data[11]
set_location_assignment PIN_E18 -to cf_data[12]
set_location_assignment PIN_F16 -to cf_data[13]
set_location_assignment PIN_F19 -to cf_data[14]
set_location_assignment PIN_G16 -to cf_data[15]
set_location_assignment PIN_G19 -to cf_iord_n
set_location_assignment PIN_G20 -to cf_iowr_n
set_location_assignment PIN_M13 -to cf_power
set_location_assignment PIN_U20 -to cf_rfu
set_location_assignment PIN_V18 -to cf_we_n
set_global_assignment -name FITTER_EFFORT "STANDARD FIT"
set_global_assignment -name PHYSICAL_SYNTHESIS_COMBO_LOGIC ON
set_global_assignment -name PHYSICAL_SYNTHESIS_REGISTER_DUPLICATION ON
set_global_assignment -name PHYSICAL_SYNTHESIS_REGISTER_RETIMING ON
set_global_assignment -name ADV_NETLIST_OPT_SYNTH_WYSIWYG_REMAP ON
set_global_assignment -name ADV_NETLIST_OPT_SYNTH_GATE_RETIME ON
set_global_assignment -name CYCLONE_OPTIMIZATION_TECHNIQUE SPEED

set_global_assignment -name RESERVE_ALL_UNUSED_PINS_NO_OUTPUT_GND "AS INPUT TRI-STATED"
set_global_assignment -name VHDL_FILE altera_europa_support.vhd
set_global_assignment -name SOURCE_FILE ./addroundkey.vhd
set_global_assignment -name SOURCE_FILE ./mixcolumn.vhd
set_global_assignment -name SOURCE_FILE ./xor32.vhd
set_global_assignment -name SOURCE_FILE ./subbytes.vhd