--scfifo DEVICE_FAMILY="Cyclone" LPM_NUMWORDS=64 LPM_SHOWAHEAD="OFF" lpm_width=8 lpm_widthu=6 OPTIMIZE_FOR_SPEED=9 OVERFLOW_CHECKING="OFF" UNDERFLOW_CHECKING="OFF" USE_EAB="ON" aclr clock data empty full q rdreq usedw wrreq CARRY_CHAIN="MANUAL" CARRY_CHAIN_LENGTH=48 CYCLONEII_M4K_COMPATIBILITY="ON" LOW_POWER_MODE="AUTO" lpm_hint="RAM_BLOCK_TYPE=AUTO" RAM_BLOCK_TYPE="AUTO"
--VERSION_BEGIN 6.0 cbx_altdpram 2006:01:09:10:52:42:SJ cbx_altsyncram 2006:03:30:14:59:04:SJ cbx_cycloneii 2006:02:07:15:19:20:SJ cbx_fifo_common 2006:01:09:11:23:34:SJ cbx_lpm_add_sub 2006:01:09:11:17:20:SJ cbx_lpm_compare 2006:01:09:11:15:40:SJ cbx_lpm_counter 2006:03:23:14:19:24:SJ cbx_lpm_decode 2006:01:09:11:16:44:SJ cbx_lpm_mux 2006:01:09:11:16:16:SJ cbx_mgl 2006:04:14:11:14:36:SJ cbx_scfifo 2006:01:09:11:24:10:SJ cbx_stratix 2006:02:07:15:17:04:SJ cbx_stratixii 2006:03:03:09:35:36:SJ cbx_util_mgl 2006:01:09:10:46:36:SJ  VERSION_END


--  Copyright (C) 1991-2006 Altera Corporation
--  Your use of Altera Corporation's design tools, logic functions 
--  and other software and tools, and its AMPP partner logic 
--  functions, and any output files any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Altera Program License 
--  Subscription Agreement, Altera MegaCore Function License 
--  Agreement, or other applicable license agreement, including, 
--  without limitation, that your use is for the sole purpose of 
--  programming logic devices manufactured by Altera and sold by 
--  Altera or its authorized distributors.  Please refer to the 
--  applicable agreement for further details.


FUNCTION a_dpfifo_ml21 (aclr, clock, data[7..0], rreq, sclr, wreq)
RETURNS ( empty, full, q[7..0], usedw[5..0]);

--synthesis_resources = lut 14 M4K 8 
SUBDESIGN scfifo_jf21
( 
	aclr	:	input;
	clock	:	input;
	data[7..0]	:	input;
	empty	:	output;
	full	:	output;
	q[7..0]	:	output;
	rdreq	:	input;
	usedw[5..0]	:	output;
	wrreq	:	input;
) 
VARIABLE 
	dpfifo : a_dpfifo_ml21;
	sclr	: NODE;

BEGIN 
	dpfifo.aclr = aclr;
	dpfifo.clock = clock;
	dpfifo.data[] = data[];
	dpfifo.rreq = rdreq;
	dpfifo.sclr = sclr;
	dpfifo.wreq = wrreq;
	empty = dpfifo.empty;
	full = dpfifo.full;
	q[] = dpfifo.q[];
	sclr = GND;
	usedw[] = dpfifo.usedw[];
END;
--VALID FILE
